{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":8,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXM-N9"]
[]
[]
[]
[]
["","","","","FCAG35BVEB / RXM35N5V1B9","FCAG35BVEB / RXM35N2V1B9","FCAG50BVEB / RXM50N2V1B9","FCAG60BVEB / RXM60N2V1B9"]
["Capacità di Raffrescamento","Nom.","","kW","3.50","3.50","5.00","5.70"]
["Capacità di riscaldamento","Nom.","","kW","4.20","4.20","6.00","7.00"]
["Efficienza nominale","EER","","","3.72","3.72","3.58","3.31"]
["","COP","","","3.77","3.77","3.70","3.38"]
["","Consumo energetico annuale","","kWh","470","470","698","861"]
["","Classe energetica","Raffreddamento","","A","A","A","A"]
["","","Riscaldamento","","A","A","A","C"]
["Raffrescamento ambienti","Classe di efficienza energetica","","","A++","A++","A++","A++"]
["","Capacità","Pdesign","kW","3.50","3.50","5.00","5.70"]
["","SEER","","","6.35","6.35","6.54","6.40"]
["","Consumi energetici annuali","","kWh/a","193","193","268","312"]
["Riscaldamento ambienti (Condizioni climatiche medie)","Classe di efficienza energetica","","","A++","A++","A+","A+"]
["","Capacità","Pdesign","kW","3.32","3.32","4.36","4.71"]
["","SCOP/A","","","4.90","4.90","4.30","4.20"]
["","Pdh Capacità di riscaldamento a -10°","","kW","","","3.86"]
["","Consumi energetici annuali","","kWh/a","948","948","1,418","1,569"]
["Note","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]