{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXS-F"]
[]
[]
[]
[]
["","","","","FVXS25FV1B (Archived)","FVXS35FV1B (Archived)","FVXS50FV1B (Archived)"]
["Schalldruckpegel","Heizen","Hoch","dB(A)","38","39","45"]
["","","Flüsterbetrieb","dB(A)","23","24","32"]
["","","Niedrig","dB(A)","26","27","36"]
["","Kühlung","Flüsterbetrieb","dB(A)","23","24","32"]
["","","Niedrig","dB(A)","26","27","36"]
["","","Hoch","dB(A)","38","39","44"]
["","","Nom.","dB(A)","32","33","40"]
["","Kühlung","Nom.","dB(A)","32","33","40"]
["Standardzubehör","Installationsanleitung","","","1","1","1"]
["","Bedienungsanleitung","","","1","1","1"]
["","Infrarotfernbedienung","","","1","1","1"]
["","Batterien","","","2","2","2"]
["","Fernbedienungshalterung","","","1","1","1"]
["","Kondensatschlauch","","","1","1","1"]
["","Luftzufuhrfilter","","","","1","1"]
["","Wärmeisolierungsband","","","2","2","2"]
["Regelungssysteme","Infrared remote control","","","ARC452A1","ARC452A1","ARC452A1"]
["Rohrleitungsanschlüsse","Flüssigkeit","AD","mm","6.35","6.35","6.35"]
["","Gas","AD","mm","9.5","9.52","12.7"]
["","Ableitung","","","20","20","20"]
["Sound power level","Kühlung","","dB(A)","52","52","60"]
["","Heizen","","dB(A)","52","52","60"]
["Abmessungen","Maßeinheit","Breite","mm","700","700","700"]
["","","Tiefe","mm","210","210","210"]
["","","Höhe","mm","600","600","600"]
["Gehäuse","Farbe","","","Weiß","Weiß","Weiß"]
["Gewicht","Maßeinheit","","kg","14","14","14"]
["Power supply","Phase","","","1~","1~","1~"]
["","Frequenz","","Hz","50","50","50"]
["","Bezeichnung","","","V1","V1","V1"]
["","Spannung","","V","220-240","220-240","220-240"]
["Hinweise","","","","(1) - 220 V","(1) - 220 V"]
["","","","","(2) - 230 V","(2) - 230 V"]
["","","","","(3) - 240 V","(3) - 240 V"]
["Standardzubehör","Luftreinigungsfilter","","","2"]
["Hinweise","","","","(4) - Bei Anschluss an einem Multi-Außengerät lesen Sie bitte die technischen Gerätedaten des anzuschließenden Multi-Außengeräts."]