{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1E53C"]
[]
[]
[]
[]
["","","","","BRC1E53C7"]
["Verpackung","Material","","","Karton_"]
["","Gewicht","","kg","0.05"]
["Umgebungstemperatur","Relative Luftfeuchte <","","%","95"]
["Abmessungen","Versandpaket","Breite","mm","160"]
["","","Höhe","mm","55"]
["","","Tiefe","mm","150"]
["","Maßeinheit","Breite","mm","120"]
["","","Tiefe","mm","19"]
["","","Höhe","mm","120"]
["Gehäuse","Tastenabdeckung","","","Nein"]
["","Farbe","","","Reinweiß"]
["","Betriebs-LED","Farbe","","Grün"]
["LCD","Typ","","","Voller Punkt (160 x 255)"]
["","Hintergrundlicht","Farbe","","Weiß"]
["","Abmessungen","Breite","mm","68.85"]
["","","Höhe","mm","43.2"]
["Gewicht","Versandpaket","","kg","0.415"]
["","Maßeinheit","","kg","0.200"]
["Reserve für Stromausfall","","","","Ja (Die Uhr läuft für maximal 48 Stunden weiter)"]
["Verdrahtungsanschlüsse","Kabellänge","max.","m","500"]